How to Perform Situational Awareness Attacks, Part 1

By [**tokyoneon**](https://creator.wonderhowto.com/tokyoneon/) 09/15/2018 12:46 am

The first few minutes after [gaining access to a MacBook](https://null-byte.wonderhowto.com/how-to/hacking-macos-configure-backdoor-anyones-macbook-0184637/) are critical — but where do we begin? Using tools built into macOS, we can develop an in-depth understanding of running background processes, detect antivirus software, locate sensitive files, and fingerprint other devices on the network. All of this can be done without installing additional software or modifying any files.

What Is Situational Awareness?

During most red team engagements, after compromising a target, pentester's will often find they need to learn as much about the device and its network surroundings as possible. This is commonly referred to as "situational awareness." This is the act of gathering hardware, software, and network information about the target. This information can be used to [further compromise the target](https://null-byte.wonderhowto.com/how-to/hacking-macos-install-persistent-empire-backdoor-macbook-0184820/), [their online accounts](https://null-byte.wonderhowto.com/how-to/hacking-macos-dump-passwords-stored-firefox-browsers-remotely-0185234/), and [pivot to other devices](https://null-byte.wonderhowto.com/how-to/hacking-macos-spread-trojans-pivot-other-mac-computers-0186632/) and services within the network.

Our goal as penetration testers is to learn as much about our newly [compromised macOS device](https://null-byte.wonderhowto.com/how-to/hacking-macos-connect-macbook-backdoors-from-anywhere-world-0184653/) as possible without alerting the target to our presence. Generally, using tools built into the operating system to perform information gathering will help us evade detection. There are [many tools in macOS](https://ss64.com/osx/) that we can use to fingerprint the device, the network, and Wi-Fi networks it's connected to. The first (and possibly the most important) tool we'll be talking about is [system\_profiler](https://ss64.com/osx/system_profiler.html).

* **Don't Miss:** [**How to Configure a Backdoor on Anyone's MacBook**](https://null-byte.wonderhowto.com/how-to/hacking-macos-configure-backdoor-anyones-macbook-0184637/)

1 Discover Hardware & Software Details

The system\_profiler tool was designed to print system hardware and software configurations. It features the ability to export information in XML format and supports several degrees of output verbosity.

In most cases, system\_profiler will produce over 55,000 lines of data pertaining to the target macOS device. This data includes very specific hardware details, firewall settings, Wi-Fi adapter details, startup items, and detailed application info, to name just a few.

System\_profiler can be used without root privileges and is, therefore, an attacker's greatest tool for quickly discovering hardware and software specifications.

The following system\_profiler commands can be executed using a Terminal or [from a Netcat backdoor](https://null-byte.wonderhowto.com/how-to/hacking-macos-connect-macbook-backdoors-from-anywhere-world-0184653/). Use the **--help** argument to view the available options.

system\_profiler --help

Usage: system\_profiler [-listDataTypes]

system\_profiler [-xml] [-timeout n] [-detailLevel n]

system\_profiler [-xml] [-timeout n] [dataType1 ... dataTypeN]

-detailLevel n specifies the level of detail for the report

mini = short report (contains no identifying or personal information)

basic = basic hardware and network information

full = all available information

-listDataTypes lists all the available datatypes

-xml generates xml output instead of plain text

if redirected to a file with the extension ".spx"

the file can be opened in System Profiler.app

-timeout specifies the maximum time to spend gathering information

the default is 180 seconds, 0 means no timeout

Redirect stderr to /dev/null to suppress progress and error messages.

The system\_profiler "Datatypes" represent different components of the macOS system. For example, using the **SPFirewallDataType** argument will print the device's firewall configuration.

system\_profiler SPFirewallDataType

Firewall:

Firewall Settings:

Mode: Block all incoming connections

Firewall Logging: Yes

Stealth Mode: No

We've now learned the device has the firewall enabled and is [blocking all incoming connections](https://support.apple.com/HT201642). This small bit of information is critical to an attacker planning their next move and trying to establish persistence.

There's a **-listDataTypes** argument that can be used to view all of the available Datatypes.

system\_profiler -listDataTypes

Available Datatypes:

SPParallelATADataType

SPUniversalAccessDataType

SPApplicationsDataType

SPAudioDataType

SPBluetoothDataType

SPCameraDataType

SPCardReaderDataType

SPComponentDataType

SPiBridgeDataType

SPDeveloperToolsDataType

SPDiagnosticsDataType

SPDisabledSoftwareDataType

SPDiscBurningDataType

SPEthernetDataType

SPExtensionsDataType

SPFibreChannelDataType

SPFireWireDataType

SPFirewallDataType

SPFontsDataType

SPFrameworksDataType

SPDisplaysDataType

SPHardwareDataType

SPHardwareRAIDDataType

SPInstallHistoryDataType

SPNetworkLocationDataType

SPLogsDataType

SPManagedClientDataType

SPMemoryDataType

SPNVMeDataType

SPNetworkDataType

SPPCIDataType

SPParallelSCSIDataType

SPPowerDataType

SPPrefPaneDataType

SPPrintersSoftwareDataType

SPPrintersDataType

SPConfigurationProfileDataType

SPRawCameraDataType

SPSASDataType

SPSerialATADataType

SPSPIDataType

SPSmartCardsDataType

SPSoftwareDataType

SPStartupItemDataType

SPStorageDataType

SPSyncServicesDataType

SPThunderboltDataType

SPUSBDataType

SPNetworkVolumeDataType

SPWWANDataType

SPAirPortDataType

Multiple Datatypes can be used simultaneously. Below, I'm printing the MacBook's OS version and network info.

system\_profiler SPSoftwareDataType SPNetworkDataType

Software:

System Software Overview:

System Version: macOS 10.13.6 (17G65)

Kernel Version: Darwin 17.7.0

Boot Volume: macOS

Boot Mode: Normal

Computer Name: tokyoneon’s MacBook Air

User Name: tokyoneon (tokyoneon)

Secure Virtual Memory: Enabled

System Integrity Protection: Enabled

Time since boot: 1:27

Network:

Wi-Fi:

Type: AirPort

Hardware: AirPort

BSD Device Name: en0

IPv4 Addresses: 192.168.1.98

IPv4:

AdditionalRoutes:

DestinationAddress: 192.168.1.98

SubnetMask: 255.255.255.255

DestinationAddress: 169.254.0.0

SubnetMask: 255.255.0.0

Addresses: 192.168.1.98

ARPResolvedHardwareAddress: xx:xx:xx:xx:xx:xx

ARPResolvedIPAddress: 192.168.1.1

Configuration Method: DHCP

ConfirmedInterfaceName: en0

Interface Name: en0

Network Signature: IPv4.Router=192.168.1.1;IPv4.RouterHardwareAddress=xx:xx:xx:xx:xx:xx

Router: 192.168.1.1

Subnet Masks: 255.255.255.0

IPv6:

Configuration Method: Automatic

DNS:

Server Addresses: 192.168.1.1

DHCP Server Responses:

Domain Name Servers: 192.168.1.1

Lease Duration (seconds): 0

DHCP Message Type: 0x05

Routers: 192.168.1.1

Server Identifier: 192.168.1.1

Subnet Mask: 255.255.255.0

Ethernet:

MAC Address: xx:xx:xx:xx:xx:xx

Media Options:

Media Subtype: Auto Select

Proxies:

Exceptions List: \*.local, 169.254/16

FTP Passive Mode: Yes

Service Order: 0

Bluetooth PAN:

Type: Ethernet

Hardware: Ethernet

BSD Device Name: en2

IPv4:

Configuration Method: DHCP

IPv6:

Configuration Method: Automatic

Proxies:

Exceptions List: \*.local, 169.254/16

FTP Passive Mode: Yes

Service Order: 1

Thunderbolt Bridge:

Type: Ethernet

Hardware: Ethernet

BSD Device Name: bridge0

IPv4:

Configuration Method: DHCP

IPv6:

Configuration Method: Automatic

Proxies:

Exceptions List: \*.local, 169.254/16

FTP Passive Mode: Yes

Service Order: 2

When using the system\_profiler without any arguments, it will use all of the available Datatypes. This will produce an enormous amount of data and can take several minutes to complete.

2 Identify Devices on the Network

The [Address Resolution Protocol](https://en.wikipedia.org/wiki/Address_Resolution_Protocol), known commonly as ARP, translates physical ([MAC](https://en.wikipedia.org/wiki/MAC_address)) addresses into IP addresses. Computers cache ARP information in "ARP tables," which aid routers and devices on the network in quickly locating each other.

The **arp** command can be used to print the macOS device's ARP table and discover devices on the network without performing a single Nmap scan.

arp -i en0 -l -a

Neighbor Linklayer Address Expire(O) Expire(I) Netif Refs Prbs

192.168.1.1 xx:xx:xx:xx:xx:xx 1m36s 1m36s en0 1

192.168.1.79 xx:xx:xx:xx:xx:xx expired 1m18s en0 1

192.168.1.102 xx:xx:xx:xx:xx:xx expired 1m20s en0 1

The **-i** argument is used to specifies the Wi-Fi interface while **-l** prints the output data in a more human-readable format. To print all of the ARP table entries, use the **-a** argument.

We've discovered several devices on the network. The MAC addresses have been redacted but this information can be used to identify operating systems and hardware details